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Display
· 63*192 Full Dot
· Natural Textbook Display
· Algebraic input method: Natural V.P.A.M. 
· No. of figures/lines 17/1+10/1
· Icon Menu
· 4-gradation display
· Display of mantissa exponent	10+2
Memory
· Replay function 
· 9 Variables memory 
Mathematics
· 540+ Functions
· 47 Scientific constants
· 40 Metric conversions
· 24 Parenthesis levels
· Fractional arithmetic
· Angle unit (DEG/RAD/GRAD)
· Angel unit conversion (DEG/RAD/GRAD)
· Coordinate transformation Pol ÷ Rec
· Trigonometric functions sin/cos/tan/sin-1/cos-1/tan-1
· Hyperbolic functions sinh/cosh/tanh/sinh-1/cosh-1/tanh-1
· Exponential, logarithmic (In, 10x, ex)
· Mathematical functions √, x², x-1, 1/x, x!,  xy, x1/y
· Base-n calculations (hexadecimal/decimal/binary/octal)
· Logical operators (AND/OR/...)
· Sexagesimal < > decimal
· Percentage calculation
· Prime factorization
· Engineering notation ENG/ENG
· Calculation with engineering symbols
· Complex number calculations
· Random number generator
· Calculation of min/max of a quadratic function
· 4x4 Matrix calculations / Vector calculation
· Equation solver
· Inequation
· Table function f(x) & g(x)


Statistics
· Sum of ∑x, ∑x², 
· Sum of ∑x, ∑y, ∑x², ∑y², ∑x*y  
· Standard deviation 
· Distribution
· Regression
· Math box
· Permutation (nPr), Combination (nCr)
Differential and integral calculus
· Numerical integration calculus
· Numerical differential calculus
Other
· English menu language
· Spreadsheet
· QR code function
· Hardcase
· Automatic shutdown 
· Energy supply: Solar + Battery  (1x LR44)
· Dimension (H x W x D in mm) 10,7 x 77 x 162
· Weight 95g
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